Audible Warnings Components. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Audio Alarm Module | Behind the RH instrument panel near the RH front speaker | -- | Audible Warnings Connector End Views
Combination Switch | On the steering column | -- | --
Fuse Block 2 | Under the LH instrument panel | Power and Grounding Component Views in Wiring Systems | --
Headlamp Relay 2 | RH instrument panel behind the instrument panel compartment in front of the blower motor | Lighting Systems Component Views in Lighting | HVAC Connector End Views in HVAC - System Manual
Ignition Key Warning Switch | RH side of the steering column on the ignition switch | -- | --
Instrument Panel Cluster Assembly | LH instrument panel | -- | --
C3 (13 Terminals) | Instrument panel harness to the instrument panel cluster assembly behind the instrument panel cluster assembly | Instrument Panel, Gages, and Console Component Views | Audible Warnings Connector End Views
LH Door Jamb Switch (2 Door) | Lower the LH B-Pillar | Lighting Systems Component Views in Lighting | --
LH Front Door Jamb Switch (4-Door) | Lower LH B-Pillar | Lighting Systems Component Views in Lighting | --
Seat Belt Switch | In the driver's seat belt buckle on the driver's seat adjuster | -- | --
C200 (22 Cavities) | Main harness to the instrument panel harness, LH instrument panel near fuse block 2 | Harness Routing Views in Wiring Systems | --
C201 (16 Cavities) | Main harness to the instrument panel harness, LH instrument panel near fuse block 2 | Harness Routing Views in Wiring Systems | --
C211 (16 Cavities) | Instrument panel harness to the floor harness, RH instrument panel near the A-pillar | Harness Routing Views in Wiring Systems | --
C301 (6 Cavities) (2-Door) | Floor harness to the sub-floor harness behind the LH rear passenger compartment trim panel | Harness Routing Views in Wiring Systems | --
G200 | Behind the LH instrument panel above fuse block 2 | Power and Grounding Component Views in Wiring Systems | --
G202 | Behind the center instrument panel on the bulkhead | Power and Grounding Component Views in Wiring Systems | --
G300 | LH rear passenger compartment behind the trim panel | Power and Grounding Component Views in Wiring Systems | --
P200 | LH rear engine compartment on the bulkhead near the brake master cylinder | Power and Grounding Component Views in Wiring Systems | --
P201 | RH rear engine compartment on the bulkhead near the battery | Power and Grounding Component Views in Wiring Systems | --
P300 (2-Door) | LH A-pillar under the instrument panel behind the LH kick panel | Power and Grounding Component Views in Wiring Systems | --
S200 | Instrument panel harness approximately 1 cm (0.39 in) from the power mirror switch connector breakout | Harness Routing Views in Wiring Systems | --
S204 | Instrument panel harness near the C211 breakout | Harness Routing Views in Wiring Systems | --
S205 | Instrument panel harness approximately 12 cm (4.72 in) from the cigar lighter breakout | Harness Routing Views in Wiring Systems | --
S212 | Main harness approximately 6 cm (2.36 in) from the blower speed selector switch connector breakout | Harness Routing Views in Wiring Systems | --
S214 | Main harness approximately 10 cm (3.93 in) from the stoplamp switch connector breakout | Harness Routing Views in Wiring Systems | --
S216 | Main harness approximately 2 cm (0.78 in) from the stoplamp switch connector breakout | Harness Routing Views in Wiring Systems | --
S221 | Instrument panel harness approximately 12 cm (4.72 in) from the cigar lighter breakout | Harness Routing Views in Wiring Systems | --
S222 | Main harness approximately 10 cm (3.93 in) from the blower speed selector switch connector breakout | Harness Routing Views in Wiring Systems | --
S226 | Instrument panel harness near the radio breakout | Harness Routing Views in Wiring Systems | --
S230 | Main harness approximately 5 cm (1.96 in) from the G300 breakout | Harness Routing Views in Wiring Systems | --
S231 | Main harness approximately 1 cm (0.39 in) from the blower speed selector switch connector breakout | Harness Routing Views in Wiring Systems | --
S232 | Main harness approximately 1 cm (0.39 in) from the G200 breakout | Harness Routing Views in Wiring Systems | --
S250 | Main harness approximately 5 cm (1.96 in) from the blower motor resistor connector breakout | Harness Routing Views in Wiring Systems | --
S262 | Main harness approximately 8 cm (3.14 in) from the stoplamp switch connector breakout | Harness Routing Views in Wiring Systems | --
S272 | Main harness approximately 11 cm (4.33 in) from the G200 breakout | Harness Routing Views in Wiring Systems | --
S275 | Main harness approximately 11 cm (4.33 in) from the ignition switch connector breakout | Harness Routing Views in Wiring Systems | --
S276 | Main harness approximately 1 cm (0.39 in) from the G200 breakout | Harness Routing Views in Wiring Systems | --
S282 | Main harness near G200 breakout | Harness Routing Views in Wiring Systems | --
S283 | Main harness approximately 8 cm (3.14 in) from the daytime running lamps (DRL) control module connector breakout | Harness Routing Views in Wiring Systems | --
S300 (2-Door) | Floor harness approximately 10 cm (3.93 in) from the LH rear speaker connector breakout | Harness Routing Views in Wiring Systems | --
S306 (2-Door) | Floor harness approximately 20 cm (7.87 in) from the LH rear speaker connector breakout | Harness Routing Views in Wiring Systems | --
S404 (2-Door) | Floor harness approximately 4 cm (1.57 in) from the C406 breakout | Harness Routing Views in Wiring Systems | --
S404 (4-Door) | Floor harness approximately 4 cm (1.57 in) from the LH rear speaker connector breakout | Harness Routing Views in Wiring Systems | --
S405 | Floor harness approximately 4 cm (1.57 in) from the G300 breakout | Harness Routing Views in Wiring Systems | --
S406 (4-Door) | Floor harness approximately 4 cm (1.57 in) from the G300 breakout | Harness Routing Views in Wiring Systems | --
S425 (4-Door) | Floor harness approximately 50 cm (19.68 in) from the G300 breakout | Harness Routing Views in Wiring Systems | --