Power Mirrors Inoperative. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Outside Mirror System Check? | -- | Go to Step 2 | Go to Outside Mirrors System Check
2 | Use a J 35616-200 to backprobe the power mirror switch from cavity 7 to ground. Does the test lamp light? | -- | Go to Step 4 | Go to Step 3
3 | Repair the open in the BLK/WHT wire between fuse block 2 and the power mirror switch. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Outside Mirrors System Check | --
4 | Use a J 35616-200 to backprobe the power mirror switch from cavity 5 to B+. Does the test lamp light? | -- | Go to Step 6 | Go to Step 5
5 | Repair the open in the BLK wire between the power mirror switch and G200. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Outside Mirrors System Check | --

6

1. Turn the ignition switch to the LOCK position.
2. Disconnect the power mirror switch connector and the left front power mirror switch assembly connector.
3. Connect a J 39200 from cavity 3 of the left front power mirror switch assembly connector to cavity 6 of the power mirror switch.

Is the resistance within the specified range?

0-0.3 ohms

Go to Step 8

Go to Step 7

7 | Repair the open in the WHT wire between the power mirror switch and S238. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Outside Mirrors System Check | --
8 | Replace the power mirror switch. Is the repair complete? | -- | Go to Outside Mirrors System Check | --