Rear Door Jamb Switch Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the left tail lamp assembly from the vehicle. Refer to Tail Lamp Replacement in Lighting Systems.
2. Disconnect the rear door jamb switch electrical connector.
3. Pull the rear door jamb switch rubber cap off the switch.
4. Use a flat-bladed tool in order to gently pry the rear door jamb switch away from the body.
5. Remove the switch from the rear door jamb.

### Installation Procedure

1. Install the rear door switch to the rear door jamb by pressing the switch into place.
2. Install the door jamb switch rubber cap to the switch.
3. Connect the rear door jamb switch electrical connector.
4. Install the left tail lamp assembly to the vehicle. Refer to Tail Lamp Replacement in Lighting Systems.