Oil Level Indicator Tube Replacement. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the oil level indicator from the guide tube.
2. Remove the bolt and guide tube (1) from the cylinder block.
3. Remove the guide tube seal (3) from the oil pump body (2).

### Installation Procedure

1. Coat the new guide tube seal with new engine oil.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the new guide tube seal (3) to the cylinder block. Secure the guide tube to the cylinder block with one bolt.

Tighten
Tighten the bolt to 14 N·m (10 lb ft).

3. Install the oil level indicator to the guide tube.