Tail Lamp Replacement. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the 2 screws which secure the tail lamp (1).
2. Pull the tail lamp (1) away from the rear end panel in order to gain access to the bulb sockets.
3. Disconnect the electrical connector (2).
4. Remove the 3 bulb sockets (1, 3, 4) from the tail lamp.
5. Remove the tail lamp from the vehicle.
6. Remove the bulbs from the sockets, if necessary.

### Installation Procedure

1. Install the bulbs to the sockets, if removed.
2. Install the 3 bulb sockets (1, 3, 4) to the tail lamp.
3. Connect the electrical connector (2).
4. Install the tail lamp (1) to the rear end panel. Secure the tail lamp with the 2 screws.