Wiper/Washer Rear System Check. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---

1

1. Turn ignition switch to ON.
2. Position and press the rear Wiper switch to the ON position.

Rear wiper operates.

Rear Wiper Inoperative

2

Press rear wiper switch to OFF.

Rear wiper stops in the park position.

• | Rear Wiper Always On

• | Rear Wiper Blade Does Not Park

3

Press and hold the rear washer switch.

Rear washer pump operates and rear wiper completes at least one full sweep.

• | Rear Washer Inoperative

• | Rear Wiper Inoperative

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.