Assist Handle Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

## Assist Handle Replacement 4 Door

### Removal Procedure

1. Remove the 2 screws from each assist handle (3, 8).
2. Remove the assist handles (3, 8) from the vehicle.

### Installation Procedure

Install the assist handles (3, 8) to the vehicle. Secure each handle with 2 screws.

## Assist Handle Replacement 2 Door -Rear

### Removal Procedure

1. Remove the 2 screws which secure the assist handle (1).
2. Remove the assist handle (1) from the vehicle.

### Installation Procedure

Install the assist handle (1) to the vehicle (1). Secure the handle with 2 screws.