Headlamps Inoperative - Low Beams. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Headlight System Check? | -- | Go to Step 2 | Go to Headlight System Check
2 | Are both low beams inoperative? | -- | Go to Step 3 | Go to Headlamps Inoperative - One Lamp

3

1. Disconnect the combination switch connector.
2. Connect a J 36169-A fused jumper wire from the combination switch connector cavity 10 to ground.

Do the low beams operate?

--

Go to Step 4

Go to Step 5

4 | Replace the combination switch. Is the replacement complete? | -- | Go to Headlight System Check | --
5 | Repair the open RED/WHT wire between cavity 10 of the combination switch connector and S243. Refer to Wiring Repairs in Wiring systems. Is the repair complete? | -- | Go to Headlight System Check | --