Rear Door Lock Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the 14 plastic retaining clips which secure the rear door interior trim panel (1).
2. Remove the rear door interior trim panel (1).
3. Remove the lock cylinder control rod (3) from the rear door lock.
4. Remove the rear door handle rod from the rear door lock (1).
5. Remove the 3 rear door lock mounting screws.
6. Remove the rear door lock (1) from the rear door.

### Installation Procedure

1. Install the rear door lock (1) to the rear door. Secure the rear door lock (1) with the 3 screws.
2. Install the rear door handle rod (4) to the rear door lock.
3. Inspect the water deflector for tears or holes.
4. Use waterproof tape on both sides of the deflector, if needed.
5. Apply adhesive to the back of the water deflector.
6. Install the water deflector to the rear door.
7. Install the rear door interior trim panel (1) to the rear door (2). Secure the trim panel (1) with the 14 panel plastic retaining clips.