Headlight System Check. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 | Turn the combination switch to the LO position. | Both headlights operate at low intensity. | Headlamps Inoperative - Low Beams Headlamps Inoperative - One Lamp Low and High Beams Headlamps Inoperative
2 | Push the combination switch to the HI position. | Both headlights operate at high intensity and the high beam indicator lights. | Headlamps Inoperative - High Beams Headlamps Inoperative - One Lamp Low and High Beams Headlamps Inoperative High Beam Indicator Inoperative

3

1. Turn the combination switch to the LO position.
2. Pull the combination switch to the PASS position and release.

Both headlights operate at high intensity while the combination switch is in the PASS position.

Headlamps Flash to Pass Inoperative

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.