Backup Lamp Bulb Replacement. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the 2 screws which secure the the bottom of the taillamp (1).
2. Remove the taillamp (1) by using the following procedure:

2.1. | Pull upward

2.2. | Pull rearward

3. Remove the backup lamp bulb socket (4) from the taillamp.
4. Remove the backup lamp bulb from the backup lamp bulb socket (4).

### Installation Procedure

1. Install the backup lamp bulb to the backup lamp bulb socket (4).
2. Install the backup lamp bulb socket (4) to the taillamp.
3. Install the taillamp (1) to the vehicle. Secure the taillamp (1) with the 2 screws.