Fastener Tightening Specifications. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Conditioning Flexible Hose Bolts | 15 N·m | 11 lb ft
Cooling Fan Nuts | 11 N·m | 97 lb in
Coolant Pump Bolts | 12 N·m | 106 lb in
Crankshaft Pulley Bolts | 16 N·m | 12 lb ft
Engine Oil Level Indicator Tube Mounting Bolt | 11 N·m | 97 lb in
Fan Clutch Nuts | 11 N·m | 97 lb in
Generator Mounting Bracket Bolt | 23 N·m | 17 lb ft
Generator Upper Mounting Bolt | 27 N·m | 20 lb ft
Coolant Intake Pipe Bolt | 11 N·m | 97 lb in
Outlet Support Pipe Bolt | 11 N·m | 97 lb in
Power Steering Fluid Reservoir Bolts | 15 N·m | 11 lb ft
Radiator Bolts | 10 N·m | 89 lb in
Shroud Bolts | 11 N·m | 97 lb in
Thermostat Cap Bolts | 16 N·m | 12 lb ft