Detent Lever and Manual Shaft Installation. Pontiac Sun Runner - 2WD (Canada) 1997

For 1990-2009 cars

1. Install the manual shaft seal (142), if necessary.
2. Install the manual shaft. The Identification groove must be on the outside.
3. Install the manual shaft spring pin (143).
4. Check the manual shaft (141) for free movement.
5. Install the detent lever (140) and parking pawl actuator (123) assembly.
6. Install the manual shaft nut (144).

Tighten
Tighten the nut to 12 N·m (9 lb ft).

Refer to Fastener Notice .