Rear Window Washer Pump Replacement. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Disconnect the rear washer pump electrical connector.
2. Remove the rear washer hose from the rear washer pump.
3. Remove the rear washer pump from the washer fluid reservoir.

### Installation Procedure

1. Install the rear washer pump to the washer fluid reservoir.
2. Install the washer hose to the rear washer pump.
3. Connect the rear washer pump electrical connector.