Power Mirrors Inoperative - One. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Outside Mirrors System Check? | -- | Go to Step 2 | Go to Outside Mirrors System Check
2 | Is the left front power mirror switch assembly inoperative? | -- | Go to Step 3 | Go to Step 14

3

1. Move the power mirror select switch to the L position.
2. Use a J 35616-200 unpowered test lamp to backprobe from cavity 2 to cavity 6.
3. Move the power mirror switch to the UP position and the DOWN position.

Does the test lamp light with the switch in both positions?

--

Go to Step 5

Go to Step 4

4 | Replace the Power Mirror Switch Replacement . Is the repair complete? | -- | Go to Outside Mirrors System Check | --

5

1. Use a J 35616-200 unpowered test lamp to backprobe the power mirror switch from cavity 3 to cavity 6.
2. Move the power mirror switch to the UP position and the DOWN position.

Does the test lamp light in both directions?

--

Go to Step 7

Go to Step 6

6 | Replace the Power Mirror Switch Replacement . Is the repair complete? | -- | Go to Outside Mirrors System Check | --

7

1. Use a J 35616-200 unpowered test lamp to backprobe the power mirror switch from cavity 2 to cavity 3.
2. Move the power mirror switch to the LEFT position.

Does the test lamp light?

--

Go to Step 11

Go to Step 8

8

1. Use a J 35616-200 unpowered test lamp to backprobe the power mirror switch from cavity 3 to ground.
2. Move the power mirror switch to the LEFT position.

Does the test lamp light?

--

Go to Step 10

Go to Step 9

9 | Repair the open in the GRN wire between the power mirror switch and the left front power mirror assembly. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Outside Mirrors System Check | --
10 | Repair the open in the WHT wire between S238 and the left front power mirror assembly. Is the repair complete? | -- | Go to Outside Mirrors System Check | --

11

1. Use a J 35616-200 unpowered test lamp to backprobe from cavity 6 to cavity 3.
2. Move the power mirror switch to the DOWN position.

Does the test lamp light?

--

Go to Step 13

Go to Step 12

12 | Repair the open in the BRN wire between the power mirror switch and the left front power mirror assembly. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Outside Mirrors System Check | --
13 | Replace the left front power mirror assembly. Is the repair complete? | -- | Go to Outside Mirrors System Check | --

14

1. Move the power mirror select switch to the R position.
2. Use a J 35616-200 unpowered test lamp to backprobe from cavity 1 to cavity 6.
3. Move the power mirror switch to the L position and the R position.

Does the test lamp light in both positions?

--

Go to Step 16

Go to Step 15

15 | Replace the Power Mirror Switch Replacement . Is the repair complete? | -- | Go to Outside Mirrors System Check | --

16

1. Use a J 35616-200 unpowered test lamp to backprobe the power mirror switch from cavity 4 to cavity 6.
2. Move the power mirror switch to the UP position and the DOWN position.

Does the test lamp light in both positions?

--

Go to Step 18

Go to Step 17

17 | Replace the Power Mirror Switch Replacement . Is the repair complete? | -- | Go to Outside Mirrors System Check | --

18

1. Use a J 35616-200 unpowered test lamp to backprobe the right front power mirror switch assembly from cavity 2 to cavity 3.
2. Push the power mirror switch to the L position.

Does the test lamp light?

--

Go to Step 22

Go to Step 19

19

1. Use a J 35616-200 unpowered test lamp to backprobe the right front power mirror switch assembly from cavity 3 to ground.
2. Push the power mirror switch to the L position.

Does the test lamp light?

--

Go to Step 21

Go to Step 20

20 | Repair the open in the GRN wire between the power mirror switch and the right power mirror switch assembly. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Outside Mirrors System Check | --
21 | Repair the open in the WHT wire between S238 and the right front power mirror assembly. Is the repair complete? | -- | Go to Outside Mirrors System Check | --

22

1. Use a J 35616-200 unpowered test lamp to backprobe the power mirror switch assembly from cavity 2 to cavity 1.
2. Move the power mirror switch to the DOWN position.

Does the test lamp light?

--

Go to Step 24

Go to Step 23

23 | Repair the open in the BRN wire or the BRN/RED wire between the power mirror switch and the right front power mirror assembly. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Outside Mirrors System Check | --
24 | Replace the right front power mirror assembly. Is the repair complete? | -- | Go to Outside Mirrors System Check | --