Radio Rear Speaker Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

## Radio Rear Speaker Replacement 2 Door

### Removal Procedure

1. Remove the screw from the front seat belt trim bezel.
2. Disengage the rear quarter interior trim panel plastic clips in order to pull the rear quarter interior trim panel from the vehicle.
3. Remove the 3 speaker screws in order to remove the rear speaker (2) from the body.
4. Disconnect the rear speaker electrical connector (1).
5. Remove the rear speaker (2) from the vehicle.

### Installation Procedure

1. Connect the rear speaker electrical connector (1).
2. Install the rear speaker (2) to the vehicle. Secure the rear speaker (2) with the 3 screws.
3. Install the rear quarter interior trim panel to the vehicle. Press the rear quarter interior trim panel into place in order to engage the plastic clips.
4. Install the front seat belt trim bezel to the vehicle. Secure the front seat belt trim bezel with the screw.

## Radio Rear Speaker Replacement 4 Door

### Removal Procedure

1. Pull the rear door weatherstrip from over the rear quarter interior trim panel.
2. Disengage the rear quarter interior trim panel plastic clips in order to pull the rear quarter interior trim panel from the vehicle.
3. Remove the 3 rear speaker screws (2) in order to remove the rear speaker (3) from the body.
4. Disconnect the rear speaker electrical connector (1).
5. Remove the rear speaker (3) from the vehicle.

### Installation Procedure

1. Connect the rear speaker electrical connector (1).
2. Install the rear speaker to the vehicle. Secure the rear speaker (2) with the 3 screws.
3. Install the rear quarter interior trim panel to the vehicle. Press the rear quarter interior trim panel into place in order to engage the plastic clips.
4. Install the rear door weatherstrip.