Shift Lever Replacement - On Vehicle. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

1. Remove two screws, two plastic retainers and the rear console box from the floor.
2. Remove two screws, two plastic retainers and the front console box from the floor.
3. Remove one screw and the gearshift control lever knob (1) from the gearshift control lever.
4. Remove eight screws, the boot cover and the gearshift control lever boot (1) from the gearshift control lever.
5. Remove one clamp and the gearshift lever case boot from the gear shift lever case.
6. Remove the gearshift control lever (1) from the gearshift lever case (2) by pushing down on the gearshift control lever pivot (3) and turning counterclockwise 90 degrees (1/4 turn) and lifting up.
7. Inspect the gearshift control lever for distortion or excessive wear. Replace as necessary.
8. Inspect the gearshift control lever boot and the gearshift lever case cover boot for tears or other damage. Replace as necessary.

### Installation Procedure

1. Install the gearshift control lever into the gearshift lever case by pushing down on the shift control lever pivot and turning clockwise 90 degrees (1/4 turn) and releasing.
2. Install the gearshift lever case boot to the gearshift lever case. Secure the boot with one clamp.
3. Install the gearshift control lever boot (1) and the boot cover onto the gearshift control lever (2). Secure the boot and the cover with eight screws.
4. Install the gearshift control lever knob (1) onto gearshift control lever. Secure the knob with one screw.
5. Install the front console box to the floor. Secure the front console box with two plastic retainers and two screws.
6. Install the rear console box to the floor. Secure the rear console box with two plastic retainers and two screws.