Engine Electrical Components. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Battery | RH Rear Engine Compartment, behind Strut Tower | Instrument Panel, Gages, and Console Component Views in Instrument Panel,Gages and Consol | Data Link Communications Connector End Views in Instrument Panel,Gages and Consol
Clutch Pedal Position (CPP) Switch (Manual Transmission) | Behind LH I/P, above Powertrain Control Module (PCM) | -- | --
Fuse Block 1 | RH Engine Compartment, front of Battery | Power and Grounding Component Views | --
Fuse Block 1 C4 (2 Cavities) | Main Harness to Fuse Block 1, below Fuse Block 1 | Power and Grounding Component Views | --
Fuse Block 2 | Under LH I/P | Power and Grounding Component Views | --
Generator | RH Lower front of Engine | -- | --
Ignition Switch | On Steering Column | Power and Grounding Component Views | --
Instrument Panel Cluster assembly | LH side of the I/P | -- | --
Park/Neutral Position (PNP) Switch (3-Speed Automatic Transmission) | RH side of Transmission | -- | --
Park/Neutral Position (PNP) Switch (3-Speed Automatic Transmission) C1 | Engine Harness to PNP Switch, RH side of Transmission | -- | --
Starter Motor | Lower RH side of Engine, under Intake Manifold | -- | --
Starter Solenoid | Lower RH side of Engine, on Starter Motor | -- | --
Transmission Range Switch (4-Speed Automatic Transmission) | RH side of Transmission | -- | --
C100 (16 Cavities) | Main Harness to Engine Harness, mounted to Bracket on Bulkhead, left of Front Wiper Motor | Harness Routing Views | --
C101 (16 Cavities) | Main Harness to Engine Harness, mounted to Bracket on Bulkhead, left of Front Wiper Motor | Harness Routing Views | --
C106 (10 Cavities) (4-Speed Automatic Transmission) | Engine Harness to Transmission Harness, RH rear Engine, under Intake Manifold | Harness Routing Views | --
C200 (22 Cavities) | Main Harness to I/P Harness, LH I/P near Fuse Block 2 | Harness Routing Views | --
C201 (16 Cavities) | Main Harness to I/P Harness, LH I/P near Fuse Block 2 | Harness Routing Views | --
G106 | RH Inner Fender, near Battery | Power and Grounding Component Views | --
G107 | RH Engine, near Starter Motor | Power and Grounding Component Views | --
P200 | LH Rear Engine Compartment on Bulkhead, near Brake Master Cylinder | Harness Routing Views | --
P201 | LH Rear Engine Compartment on Bulkhead, near Battery | Harness Routing Views | --
S100 (With Cruise) | Main Harness, approximately 21 cm from front Wiper Motor connector breakout | Harness Routing Views | --
S130 | Main Harness, approximately 20 cm from Noise Suppressor Filter connector breakout | Harness Routing Views | --
S136 | engine Harness, approximately 1 cm from Distributor connector breakout | Harness Routing Views | --
S204 | I/P Harness, approximately at C211 breakout | Harness Routing Views | --
S240 (4-Door) | Main Harness, approximately 2 cm from Powertrain Control Module (PCM) connectors breakout | Harness Routing Views | --
S248 Manual Transmission | Main Harness, approximately 13 cm from Steering Column branch breakout | Harness Routing Views | --
S272 | Main Harness, approximately 11 cm from G200 breakout | Harness Routing Views | --