Engine Controls Components. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
A/C Amplifier | Behind RH I/P on Evaporator | HVAC Component Views in HVAC System Manual | HVAC Connector End Views in HVAC System Manual
Clutch Pedal Position (CPP) Switch (Manual Transmission) | Behind LH I/P, above Powertrain Control Module (PCM) | Cruise Control Component Views | --
Crankshaft Position Sensor | Lower front of Engine, front of Oil Pan | -- | --
Cruise Control Actuator | RH Engine Compartment, near Strut Tower | Cruise Control Component Views in Cruise Control | --
Data Link Connector - On Board Diagnostics II (DLC-OBD II) | LH I/P, Left of Center Console on Knee Bolster | Data Link Communications Component Views | Data Link Communications Component Views
Distributor | Top rear of Engine | Engine Controls Component Views | Powertrain Control Module Connector End Views
Duty Check Data Link Connector (DLC) 1 | RH Engine Compartment, behind RH Headlamp | Data Link Communications Component Views | --
Duty Check Data Link Connector (DLC) 2 (4-Speed Automatic Transmission) | RH Engine Compartment, behind RH Headlamp | Data Link Communications Component Views |
Engine Coolant Temperature (ECT) Sensor | RH side of Engine in Thermostat Housing | Engine Controls Component Views | --
Evaporative (EVAP) Canister Purge Valve | RH front Engine, on Intake Manifold | Engine Controls Component Views | --
Evaporative (EVAP) Canister Vent Control Valve | RH Engine Compartment, near Fuse Block 1 | -- | --
Evaporative (EVAP) Tank Pressure Control Solenoid Vacuum Valve | RH Engine Compartment, near Fuse Block 1 | -- | --
Exhaust Gas Recirculation (EGR) Solenoid Vacuum Valve | RH front Engine, on Intake Manifold | Engine Controls Component Views | --
Four Wheel Drive Switch | Top of Transfer Case | Antilock Brake System Component Views in ABS | --
Fuel Injector #1 | Top RH side of Engine | Engine Controls Component Views | --
Fuel Injector #2 | Top RH side of Engine | Engine Controls Component Views | --
Fuel Injector #3 | Top RH side of Engine | Engine Controls Component Views | --
Fuel Injector #4 | Top RH side of Engine | Engine Controls Component Views | --
Fuel Level Sensor | In Fuel Tank | Engine Controls Component Views | --
Fuel Pump | In Fuel Tank | Engine Controls Component Views | --
Fuel Pump Relay | Center I/P, behind Blower Speed Selector Switch | Engine Controls Component Views |
Fuel Tank Pressure Sensor | In Fuel Tank | Engine Controls Component Views | --
Fuse Block 1 | RH Engine Compartment, front of Battery | Power and Grounding Component Views | --
Fuse Block 1 - C1 (3 Cavities) | Main Harness to Fuse Block 1, below Fuse Block 1 | Power and Grounding Component Views | --
Fuse Block 2 | Under LH I/P | Power and Grounding Component Views | --
Generator | RH Lower front of Engine | -- | --
Heated Oxygen Sensor 1 (HO2S1) | LH rear of Engine, in Exhaust Manifold | Engine Controls Component Views | --
Heated Oxygen Sensor 2 (HO2S2) | Below Vehicle after Three-Way Catalytic Converter (TWC) | Engine Controls Component Views | --
Idle Air Control (IAC) Valve | RH Engine, below Throttle Body | -- | --
Ignition Switch | On Steering Column | Power and Grounding Component Views | --
Instrument Panel Cluster Assembly | LH I/P | -- | --
Instrument Panel Cluster Assembly C1 (16 Terminals) | I/P Harness to I/P Cluster Assembly, behind I/P Cluster Assembly | Instrument Panel, Gages, and Console Component Views in Instrument Panel,Gages and Consol | --
Instrument Panel Cluster Assembly C3 (13 Terminals) | I/P Harness to I/P Cluster Assembly, behind I/P Cluster Assembly | Instrument Panel, Gages, and Console Component Views in Instrument Panel,Gages and Consol | --
Intake Air Temperature (IAT) Sensor | RH front Engine below Throttle Body | Engine Controls Component Views | --
Main Relay | Center I/P, behind Blower Speed Selector Switch | Engine Controls Component Views |
Manifold Absolute Pressure (MAP) Sensor | Rear Engine Compartment, on Bulkhead | Engine Controls Component Views | --
Mass Air Flow (MAF) Sensor | LH Front Engine compartment, on Air Cleaner (ACL) Housing | Engine Controls Component Views | --
Noise Suppressor Filter | LH Front Engine Compartment, below Front Wiper Motor | Engine Controls Component Views |
Oil Pressure Switch | LH Engine, above Oil Filter | Instrument Panel, Gages, and Console Component Views in Instrument Panel,Gages and Consol | --
Overdrive Switch (4-Speed Automatic Transmission) | Center Console, mounted in Manual Selector Lever | -- | --
Park/Neutral Position (PNP) Switch (3-Speed Automatic transmission) | RH side of Transmission | -- | --
Park/Neutral Position (PNP) Switch (3-Speed Automatic transmission) - C1 (2 Cavities) | Engine Harness to PNP Switch, RH side of Transmission | -- | --
Powertrain Control Module (PCM) | Under LH I/P, left of Steering Column | Engine Controls Component Views | --
Powertrain Control Module (PCM) - (3 Speed Automatic and Manual Transmissions) - C1 (22 Cavities) | Main Harness to PCM, behind I/P left of Steering Column | Engine Controls Component Views | --
Powertrain Control Module (PCM) - (3 Speed Automatic and Manual Transmissions) - C2 (16 Cavities) | Main Harness to PCM, behind I/P left of Steering Column | Engine Controls Component Views | --
Powertrain Control Module (PCM) - (3 Speed Automatic and Manual Transmissions) - C3 (26 Cavities) | Main Harness to PCM, behind I/P left of Steering Column | Engine Controls Component Views | --
Powertrain Control Module (PCM) - (4-Speed Automatic Transmission) - C1 (22 Cavities) | Main Harness to PCM, behind I/P left of Steering Column | Engine Controls Component Views | --
Powertrain Control Module (PCM) - (4-Speed Automatic Transmission) - C2 (12 Cavities) | Main Harness to PCM, behind I/P left of Steering Column | Engine Controls Component Views | --
Powertrain Control Module (PCM) - (4-Speed Automatic Transmission) - C3 (16 Cavities) | Main Harness to PCM, behind I/P left of Steering Column | Engine Controls Component Views | --
Powertrain Control Module (PCM) - (4-Speed Automatic Transmission) - C4 (26 Cavities) | Main Harness to PCM, behind I/P left of Steering Column | Engine Controls Component Views | --
Power/Normal Switch (4-Speed Automatic Transmission) | In Center Console, right of Manual Selector Lever | -- | --
Power Steering Pressure Switch | Lower LH Engine, in Power Steering Pump | Engine Controls Component Views | --
Shift Solenoid No. 1 (4-Speed Automatic Transmission) | In Transmission, attached to Valve Body | -- | --
Shift Solenoid No. 2 (4-Speed Automatic Transmission) | In Transmission, attached to Valve Body | -- | --
Starter Motor | Lower RH side of Engine, under Intake Manifold | -- | --
Stoplamp Switch | Under LH I/P, above Brake Pedal | Lighting Systems Component Views in Lighting Systems | --
Throttle Position (TP) Sensor | On Throttle Body | Engine Controls Component Views | Powertrain Control Module Connector End Views
Torque Converter Clutch (TCC) Relay (3-Speed Automatic Transmission) | RH Engine Compartment, in front of Battery | -- | --
Torque Converter Clutch (TCC) Solenoid (Automatic Transmission) | In Transmission, attached to Valve Body | -- | --
Transmission Range Switch (4-Speed Automatic Transmission) | RH side of Transmission | -- | --
Vehicle Speed Sensor (VSS) (4-Speed Automatic Transmission) | LH side of Transmission, in Adapter Case | -- | --
C100 (16 cavities) | Main Harness to Engine Harness, mounted to Bracket on Bulkhead, left of Front Wiper Motor | Harness Routing Views | --
C101 (16 Cavities) | Main Harness to Engine Harness, mounted to Bracket on Bulkhead, left of Front Wiper Motor | Harness Routing Views | --
C102 (6 Cavities) (3-Speed Automatic Transmission) | Main Harness to Engine Harness, mounted to Bracket on Bulkhead, left of Front Wiper Motor | Harness Routing Views | --
C102 (4 Cavities) (Manual and 4-Speed Automatic Transmissions) | Main Harness to Engine Harness, mounted to Bracket on Bulkhead, left of Front Wiper Motor | Harness Routing Views | --
C103 (12 Cavities) (Manual and 4-Speed Transmissions) | Main Harness to Engine Harness, mounted to Bracket on Bulkhead, left of Front Wiper Motor | Harness Routing Views | --
C104 (6 Cavities) (Manual and 3-Speed Automatic Transmissions) | Engine Harness to Transmission Harness, under Intake Manifold | Harness Routing Views | --
C104 (9 Cavities) (4-Speed Automatic Transmission) | Engine Harness to Transmission Harness, under Intake Manifold | Harness Routing Views | --
C105 (12 Cavities) | Engine Harness to Injector Harness, RH front of Engine | Harness Routing Views | --
C106 (10 Cavities) (4-Speed Automatic Transmission) | Engine Harness to Transmission Harness, RH rear Engine, under Intake Manifold | Harness Routing Views | --
C200 (22 Cavities) | Main Harness to I/P Harness, LH I/P near Fuse Block 2 | Harness Routing Views | --
C201 (16 Cavities) | Main Harness to I/P Harness, LH I/P near fuse Block 2 | Harness Routing Views | --
C202 (22 Cavities) | Main Harness to Floor harness, LH I/P near G200 | Harness Routing Views | --
C211 (16 Cavities) | I/P Harness to Floor Harness, LH I/P, near A-Pillar | Harness Routing Views | --
C212 (10 Cavities) | Main Harness to A/C Amplifier Jumper Harness, RH I/P, behind I/P Compartment | Harness Routing Views | --
C213 (6 Cavities) | I/P Harness to Shift Illumination Jumper Harness, Center I/P | Harness Routing Views | --
C302 (6 Cavities) | Floor Harness to Sub-Floor Harness, behind LH Rear Passenger Compartment Trim Panel | Harness Routing Views | --
C400 (12 Cavities) | Floor Harness to Rear Lamp Harness, behind LH Rear Wheelhousing | Harness Routing Views | --
C401 (6 Cavities) (2-Door) | Floor Harness to Rear Lamp Harness, behind LH Rear Wheelhousing | Harness Routing Views | --
C401 (10 Cavities) (4-Door) | Floor Harness to Rear Lamp Harness, behind LH Rear Wheelhousing | Harness Routing Views | --
C411 (3 Cavities) (4-Door) | Rear Lamp Harness to Fuel Pressure Sensor Jumper Harness, under rear of Vehicle above Fuel Tank | Harness Routing Views | --
G101 | On Bulkhead behind Distributor | Power and Grounding Component Views | --
G102 | RH Rear of Engine near Distributor | Power and Grounding Component Views | --
G103 | RH Rear Engine Compartment mounted to Intake Manifold | Power and Grounding Component Views | --
G200 | Behind LH I/P, above Fuse Block 2 | Power and Grounding Component Views | --
G201 | Behind RH I/P, near Blower Assembly | Power and Grounding Component Views | --
G202 | Behind Center I/P on Bulkhead | Power and Grounding Component Views | --
G300 (4-Door) | LH Rear Passenger Compartment, behind Trim Panel | Power and Grounding Component Views | --
G300 (2-Door) | LH Rear Passenger Compartment, behind Trim Panel | Power and Grounding Component Views | --
G400 | Inside Rear Door near License Plate Lamps | Power and Grounding Component Views | --
G402 (2-Door) | Rear Lamp Harness, behind LH Rear Wheelhousing | Power and Grounding Component Views | --
P200 | LH Rear Engine Compartment on Bulkhead, near Brake Master Cylinder | Harness Routing Views | --
P201 | RH Rear Engine Compartment on Bulkhead, near Battery | Harness Routing Views | --
P300 (2-Door) | LH A-Pillar, under I/P, behind LH Kick Panel | Harness Routing Views | --
P401 | Rear of Vehicle, right of LH Frame Rail | Harness Routing Views | --
S106 | Main Harness, approximately 10 cm from Noise Suppressor Filter connector breakout | Harness Routing Views | --
S107 | Engine Harness, Approximately 10 cm from C104 breakout | Harness Routing Views | --
S108 (4-Speed Automatic transmission) | Transmission Harness, near 4WD Switch breakout | Harness Routing Views | --
S112 | Main Harness, Approximately 2 cm from P200 | Harness Routing Views | --
S122 | Engine Harness, approximately 4 cm from Crankshaft Position Sensor connector breakout | Harness Routing Views | --
S125 | Engine harness, approximately 4 cm from Starter Motor connector breakout | Harness Routing Views | --
S128 | Injector Harness, near C105 breakout | Harness Routing Views | --
S129 | Injector Harness, near Idle Air Control (IAC) Valve connector breakout | Harness Routing Views | --
S130 | Main Harness, approximately 20 cm from Noise Suppressor Filter connector breakout | Harness Routing Views | --
S131 | Main Harness, approximately 19 cm from P201 | Harness Routing Views | --
S132 | Main Harness, approximately 7 cm from Noise Suppressor Filter connector breakout | Harness Routing Views | --
S133 | Main Harness, near Heated Oxygen Sensor 1 (HO2S1) connector breakout | Harness Routing Views | --
S139 | Main Harness, approximately 10 cm from Noise Suppressor Filter connector breakout | Harness Routing Views | --
S140 | Main Harness, approximately 6 cm from Noise Suppressor Filter connector breakout | Harness Routing Views | --
S141 | Main Harness, approximately 11 cm from P200 | Harness Routing Views | --
S142 (3-Speed Automatic Transmission) | Main Harness, approximately 8 cm from P200 | Harness Routing Views | --
S204 | I/P Harness, approximately at C211 breakout | Harness Routing Views | --
S208 | Main Harness, approximately 18 cm from Ignition Switch connector breakout | Harness Routing Views | --
S210 | Main Harness, approximately 12 cm from Stoplamp Switch connector breakout | Harness Routing Views | --
S215 | Main Harness, near Powertrain Control Module (PCM) connector C2 breakout | Harness Routing Views | --
S216 | Main Harness, approximately 2 cm from Stoplamp Switch connector breakout | Harness Routing Views | --
S218 | Main harness, near G200 breakout | Harness Routing Views | --
S219 | Main Harness, approximately 10 cm from Daytime Running Lamps (DRL) Control Module connector breakout | Harness Routing Views | --
S220 | Main Harness, approximately 1 cm from Blower Speed Selector switch connector breakout | Harness Routing Views | --
S222 | Main Harness, approximately 10 cm from Blower Speed Selector Switch connector breakout | Harness Routing Views | --
S223 | Main Harness, near Fuse Block 2 | Harness Routing Views | --
S226 | I/P Harness, approximately at Radio breakout | Harness Routing Views | --
S227 | Main Harness, approximately 8 cm from Stoplamp Switch connector breakout | Harness Routing Views | --
S230 | Main Harness, approximately 5 cm from G300 breakout | Harness Routing Views | --
S234 (4-Speed Automatic Transmission) | In Manual Selector Lever Harness | Harness Routing Views | --
S241 | Main Harness, approximately 2 cm from Powertrain Control Module (PCM) connector breakout | Harness Routing Views | --
S248 (Manual Transmission) | Main Harness, approximately 13 cm from steering column branch breakout | Harness Routing Views | --
S251 | Main Harness, approximately 5 cm from Stoplamp Switch connector breakout | Harness Routing Views | --
S254 | Main Harness, approximately 10 cm from G200 breakout | Harness Routing Views | --
S260 | Main Harness, approximately 4 cm from Stoplamp Switch connector breakout | Harness Routing Views | --
S262 | Main Harness, approximately 8 cm from Stoplamp Switch connector breakout | Harness Routing Views | --
S264 | Main Harness, approximately 18 cm from Blower Speed Selector Switch connector breakout | Harness Routing Views | --
S272 | Main Harness, approximately 11 cm from G200 breakout | Harness Routing Views | --
S275 | Main Harness, approximately 11 cm from Ignition Switch connector breakout | Harness Routing Views | --
S276 | Main Harness, approximately 1 cm from G200 breakout | Harness Routing Views | --
S285 | Main Harness, approximately 10 cm from Daytime Running Lamps (DRL) Contol Module connector breakout | Harness Routing Views | --
S286 | Main Harness, approximately 6 cm from C216 breakout | Harness Routing Views | --
S287 | Main Harness, approximately 4 cm from C203 breakout | Harness Routing Views | --
S288 | Main Harness, approximately 2 cm from G200 breakout | Harness Routing Views | --
S294 | Main Harness, approximately 10 cm from G200 breakout | Harness Routing Views | --
S295 | Main Harness, approximately 7 cm from Blower Speed Selector Switch connector breakout | Harness Routing Views | --
S296 | Main Harness, approximately 6 cm from Stoplamp Switch connector breakout | Harness Routing Views | --
S297 | Main Harness, approximately 5 cm from DRL Diode connector breakout | Harness Routing Views | --
S298 | Main Harness, approximately 2 cm from G200 breakout | Harness Routing Views | --
S299 | Main Harness, approximately 6 cm from P201 | Harness Routing Views | --
S401 | Rear Lamp Harness, near LH Rear Combination Lamp | Harness Routing Views | --
S402 | Rear Lamp Harness, near RH Rear Combination Lamp | Harness Routing Views | --
S403 | Rear Lamp Harness, near RH Rear Combination Lamp | Harness Routing Views | --
S404 (2-Door) | Floor Harness, approximately 4 cm from C406 breakout | Harness Routing Views | --
S404 (4-Door) | Floor Harness, approximately 30 cm from LH Rear Speaker connector breakout | Harness Routing Views | --
S405 | Rear Door Harness, approximately 4 cm from G300 | Harness Routing Views | --
S419 (4-Door) | Floor Harness, approximately 50 cm from G300 | Harness Routing Views | --