Data Link Communications Components. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Data Link Connector - On Board Diagnostics II (DLC-OBD) | LH instrument panel to the left of the center console of the knee bolster | Data Link Communications Component Views | Data Link Communications Connector End Views
Duty Check Data Link Connector (DLC) 1 | RH engine compartment behind the RH headlamp | Data Link Communications Component Views | Data Link Communications Connector End Views
Electronic Brake Control Module (EBCM) (with ABS) | Under the LH instrument panel to the right of the steering column | Antilock Brake System Component Views in ABS | --
C1 (32 Cavities) | Main harness to the EBCM behind the instrument panel to the right of the steering column | Antilock Brake System Component Views in ABS | --
Fuse Block 2 | Under the LH instrument panel | Power and Grounding Component Views | --
Inflatable Restraint Sensing and Diagnostic Module (SDM) | Under the center of the instrument panel | -- | SIR Connector End Views in SIR
Powertrain Control Module (PCM) | Under the LH instrument panel to the left of the steering column | Engine Controls Component Views in Engine Controls - 1.6L | Powertrain Control Module Connector End Views in Engine Controls - 1.6L
3-Speed Automatic and Manual Transmissions C1 (22 Cavities) | Main harness to the PCM, behind the instrument panel to the left of the steering column | -- | --
3-Speed Automatic and Manual Transmissions C2 (16 Cavities) | Main harness to the PCM, behind the instrument panel to the left of the steering column | -- | --
3-Speed Automatic and Manual Transmissions C3 (26 Cavities) | Main harness to the PCM, behind the instrument panel to the left of the steering column | -- | --
4-Speed Automatic and Manual Transmissions C1 (22 Cavities) | Main harness to the PCM, behind the instrument panel to the left of the steering column | -- | --
4-Speed Automatic and Manual Transmissions C2 (12 Cavities) | Main harness to the PCM, behind the instrument panel to the left of the steering column | -- | --
4-Speed Automatic and Manual Transmissions C3 (16 Cavities) | Main harness to the PCM, behind the instrument panel to the left of the steering column | -- | --
4-Speed Automatic and Manual Transmissions C4 (26 Cavities) | Main harness to the PCM, behind the instrument panel to the left of the steering column | -- | --
C201 (16 Cavities) | Main harness to the instrument panel harness, LH instrument panel near fuse block 2 | Harness Routing Views | --
C208 (5 Cavities) | Instrument panel harness to the SIR harness, LH instrument panel to the right of the steering column | Harness Routing Views | --
G103 | RH rear engine compartment mounted to the intake manifold | Power and Grounding Component Views | --
G201 | Behind the RH instrument panel near the blower assembly | Power and Grounding Component Views | --
G202 | Behind the center instrument panel on the bulkhead | Power and Grounding Component Views | --
P201 | RH rear engine compartment on the bulkhead near the battery | Harness Routing Views | --
S131 | Main harness approximately 19 cm (7.48 in) from P201 | Harness Routing Views | --
S213 | Main harness approximately 3 cm (1.18 in) from the stoplamp switch connector breakout | Harness Routing Views | --
S216 | Main harness approximately 2 cm (0.78 in) from the stoplamp switch connector breakout | Harness Routing Views | --
S220 | Main harness approximately 1 cm (0.39 in) from the blower speed selector switch connector breakout | Harness Routing Views | --
S222 | Main harness approximately 10 cm (3.93 in) from the blower speed selector switch connector breakout | Harness Routing Views | --
S275 | Main harness approximately 11 cm (4.33 in) from the ignition switch connector breakout | Harness Routing Views | --
S276 | Main harness approximately 1 cm (0.39 in) from the G200 breakout | Harness Routing Views | --
S286 | Main harness approximately 6 cm (2.36 in) from the C216 breakout | Harness Routing Views | --
S296 | Main harness approximately 6 cm (2.36 in) from the stoplamp switch connector breakout | Harness Routing Views | --
S297 | Main harness approximately 5 cm (1.96 in) from the daytime running lamps (DRL) diode connector breakout | Harness Routing Views | --