Washer Nozzle Replacement. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

Important: If a nozzle becomes plugged, apply air pressure in order to help remove the obstruction. If the nozzle remains plugged, replace the nozzle.

1. Disconnect the front washer hose (2) from the nozzle (1).
2. Remove the front washer nozzle (1) from the air inlet grille.

### Installation Procedure

1. Install the front washer nozzle (1) to the air inlet grille.
2. Connect the front washer hose (2) to the front washer nozzle (1).