High Beam Indicator Inoperative. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the headlight system check? | -- | Go to Step 2 | Go to Headlight System Check
2 | Are the high beams operational? | -- | Go to Step 3 | Go to Headlamps Inoperative - High Beams
3 | Using a J 35616-200 unpowered test lamp, backprobe connector C2, cavity 8 of the instrument panel cluster assembly to ground. Does the lamp light? | -- | Go to Step 4 | Go to Step 9
4 | Using a J 36169-A fused jumper wire, backprobe connector C2, cavity 7 of the instrument panel cluster assembly to ground. Does the high beam indicator lamp light? | -- | Go to Step 6 | Go to Step 5
5 | Test for an open in the IP cluster printed circuit using a J 39200 . Is there an open condition? | -- | Go to Step 8 | Go to Step 7
6 | Repair the open RED wire between connector C2, cavity 7 of the instrument panel cluster assembly and S244. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Headlight System Check | --
7 | Replace the high beam indicator lamp. Is the replacement complete? | -- | Go to Headlight System Check | --
8 | Replace the open IP cluster printed circuit. Is the repair complete? | -- | Go to Headlight System Check | --
9 | Repair the open WHT/BLU wire between connector C2, cavity 8 of the instrument panel cluster assembly and S116. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Headlight System Check | --