Parking Brake Indicator Switch Replacement. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Remove the negative battery cable.
2. Remove the two screws, the two clips and the parking brake lever trim bezel.
3. Remove the parking brake switch electrical connector.
4. Remove one bolt and the parking brake switch (4) from the parking brake lever assembly (5).

### Installation Procedure

1. Install the parking brake switch (4) to the parking brake lever assembly (5); secure with one bolt.
2. Install the parking brake switch electrical connector.
3. Install the parking brake lever trim bezel.
4. Secure the parking brake lever trim bezel with the two screws and the two clips.
5. Install the negative battery cable.