Power Window Inoperative - Right Side Front. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Power Windows System Check? | -- | Go to Step 2 | Go to Power Windows System Check

2

1. Use a J 35616-200 unpowered test lamp in order to backprobe the right front power window motor connector from cavity 2 to ground.
2. Depress the right front window switch in the left front power window/door lock switch to the DOWN position.

Does the test lamp light?

--

Go to Step 3

Go to Step 7

3

1. Use a J 35616-200 unpowered test lamp in order to backprobe the right front power window motor connector from cavity 1 to ground.
2. Lift the right front window switch in the left front power window/door lock switch to the UP position.

Does the test lamp light?

--

Go to Step 4

Go to Step 13

4

1. Disconnect the right front power window motor connector.
2. Connect a J 35616-200 unpowered test lamp from cavity 2 to B+.

Does the test lamp light?

--

Go to Step 5

Go to Step 17

5 | Connect a J 35616-200 unpowered test lamp form the right front power window motor connector cavity 1 to B+. Does the test lamp light? | -- | Go to Step 6 | Go to Step 20
6 | Replace the right front power window regulator. Refer to Front Side Door Window Regulator Replacement . Is the repair complete? | -- | Go to Power Windows System Check | --

7

1. Use a J 35616-200 unpowered test lamp in order to backprobe the right front power window switch connector from cavity 5 to ground.
2. Depress the right front window switch in the left front power window/door lock switch to the DOWN position.

Does the test lamp light?

--

Go to Step 8

Go to Step 9

8 | Repair the open in the RED wire between the right front power window switch and the right front power window motor. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --

9

1. Use a J 35616-200 unpowered test lamp in order to backprobe the right front power window switch connector from cavity 2 to ground.
2. Depress the right front window switch in the left front power window switch in the left front power window/door lock switch to the DOWN position.

Does the test lamp light?

--

Go to Step 10

Go to Step 11

10 | Replace the right front power window switch. Refer to Front Side Door Window Switch Replacement . Is the repair complete? | -- | Go to Power Windows System Check | --

11

1. Use a J 35616-200 unpowered test lamp in order to backprobe the left front power window/door lock switch connector from cavity 6 to ground.
2. Depress the right front window switch to the DOWN position.

Does the test lamp light?

--

Go to Step 12

Go to Step 24

12 | Repair the open in the GRN/BLK wire between the left front power window/door lock switch and the right front power window switch. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --

13

1. Use a J 35616-200 unpowered test lamp in order to backprobe the right front power window switch connector from cavity 3 to ground.
2. Lift the right front window switch in the left front power window/door lock switch to the UP position.

Does the test lamp light?

--

Go to Step 14

Go to Step 15

14 | Repair the open in the YEL wire between the right front power window switch and the right front power window motor. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --

15

1. Use a J 35616-200 unpowered test lamp in order to backprobe the right front power window switch connector from cavity 4 to ground.
2. Lift the right front window switch in the left front power window/door lock switch to the UP position.

Does the test lamp light?

--

Go to Step 10

Go to Step 16

16

1. Use a J 35616-200 unpowered test lamp in order to backprobe the left front power window/door lock switch connector from cavity 7 to ground.
2. Lift the right front window switch to the UP position.

Does the test lamp light?

--

Go to Step 12

Go to Step 24

17 | Use a J 35616-200 unpowered test lamp in order to backprobe the right front power window switch connector from cavity 5 to B+. Does the test lamp light? | -- | Go to Step 8 | Go to Step 18
18 | Use a J 35616-200 unpowered test lamp in order to backprobe the right front power window switch connector from cavity 2 to B+. Does the test lamp light? | -- | Go to Step 10 | Go to Step 19
19 | Use a J 35616-200 unpowered test lamp in order to backprobe the left front power window/door lock switch connector from cavity 6 to B+. Does the test lamp light? | -- | Go to Step 12 | Go to Step 26
20 | Use a J 35616-200 unpowered test lamp in order to backprobe the right front power window switch connector from cavity 3 to B+. Does the test lamp light? | -- | Go to Step 14 | Go to Step 21
21 | Use a J 35616-200 unpowered test lamp in order to backprobe the right front power window switch connector from cavity 4 to B+. Does the test lamp light? | -- | Go to Step 10 | Go to Step 22
22 | Use a J 35616-200 unpowered test lamp in order to backprobe the left front power window/door lock switch connector from cavity 7 to B+. Does the test lamp light? | -- | Go to Step 23 | Go to Step 26
23 | Repair the open in the RED/BLK wire between the left front power window/door lock switch and the right front power window switch. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --
24 | Use a J 35616-200 unpowered test lamp in order to backprobe the left front power door lock switch connector from cavity 10 to ground. Does the test lamp light? | -- | Go to Step 26 | Go to Step 25
25 | Repair the open in the BLU/WHT wire between the left front power window/door lock switch and fuse block 2. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --
26 | Replace the left front power window/door lock switch. Refer to Door Lock and Side Window Switch Replacement . Is the repair complete? | -- | Go to Power Windows System Check | --