Horns Components. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Combination Switch | On the steering column | -- | --
Fuse Block 2 | Under the left instrument panel | Power and Grounding Component Views in Wiring System | --
Horn Relay | Center of the instrument panel behind the blower speed selector switch | Horn Component Views | --
Left Horn | Between the grill and the radiator | -- | --
LH Horn Switch | LH side of the steering wheel | -- | --
RH Horn Switch | RH side of the steering wheel | -- | --
Supplemental Inflatable Restraint (SIR) Contact Coil | In the top of the steering column | -- | --
C3 (1 Cavity) | SIR contact coil to the horn switches in the steering wheel | -- | --
G104 | RH front inner fender near the washer fluid reservoir | Power and Grounding Component Views in Wiring Systems | --
P201 | RH rear engine compartment on the bulkhead near the battery | Power and Grounding Component Views in Wiring Systems | --
S103 | Main harness, approximately 8 cm (3.14 in) from the right horn connectors breakout | Harness Routing Views in Wiring Systems | --
S104 | Main harness, approximately 4 cm (1.57 in) from the front washer pump connector breakout | Harness Routing Views in Wiring Systems | --
S105 | Main harness, approximately 11 cm (4.33 in) from the RH headlamp connector breakout | Harness Routing Views in Wiring Systems | --
S203 | Main harness, approximately 2 cm (0.78 in) from the blower motor resistor connector breakout | Harness Routing Views in Wiring Systems | --
S251 | Main harness, approximately 5 cm (1.96 in) from the stoplamp switch connector breakout | Harness Routing Views in Wiring Systems | --
S254 | Main harness, approximately 10 cm (3.93 in) from the G200 breakout | Harness Routing Views in Wiring Systems | --