Front Seat Replacement - Bucket. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

## Front Seat Replacement - Bucket 2 Door

### Removal Procedure

1. Remove the 2 screws which secure the front seat adjuster outer trim cover.
2. Remove the front seat outer adjuster trim cover (2).
3. Remove the 4 front seat anchor bolt covers (3).
4. Disconnect the seat belt electrical connector, if equipped.
5. Remove the 4 front seat anchor bolts.
6. Remove the seat from the vehicle.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the front seat to the vehicle. Secure the front seat with the 4 anchor bolts.

Tighten
Tighten the front seat anchor bolts to 25 N·m (19 lb ft).

2. Connect the front seatbelt electrical connector.
3. Install the 4 front seat anchor bolt covers (3).
4. Install the front seat adjuster trim cover to the front seat. Secure the front seat adjuster trim cover (2) with the 2 screws.

## Front Seat Replacement - Bucket 4 Door

### Removal Procedure

1. Remove the 2 screws which secure the front seat adjuster outer trim cover screws.
2. Remove the front seat outer adjuster trim cover (2).
3. Remove the 5 front seat anchor bolt covers (4).
4. Disconnect the seat belt electrical connector, if equipped.
5. Remove the 5 front seat anchor bolts.
6. Remove the seat from the vehicle.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the front seat to the vehicle. Secure the front seat with the 5 anchor bolts.

Tighten
Tighten the anchor bolts to 25 N·m (19 lb ft).

2. Connect the front seatbelt electrical connector.
3. Install the 5 front seat anchor bolt covers (4).
4. Install the front seat adjuster trim cover to the front seat. Secure the front seat adjuster trim cover (2) with the 2 screws.