Speedometer Cable Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the instrument cluster assembly. Refer to Instrument Cluster Replacement .
2. Unhook the speedometer cable from the heater case.
3. Remove the grommet from the bulkhead.
4. Feed the speedometer cable through the bulkhead.
5. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
6. Unscrew the speedometer cable (1) from either the transfer case or the transmission.
7. Remove the speedometer cable (1) from either the transfer case or the transmission.
8. Remove the speedometer cable (1) from the clamp.
9. Remove the speedometer cable (1) from the vehicle.

### Installation Procedure

1. Attach the speedometer cable (1) to the clamp.
2. Screw the speedometer cable (1) to the transfer case or the transmission.
3. Lower the vehicle.
4. Feed the speedometer cable (1) through the bulkhead.
5. Install the grommet to the bulkhead.
6. Hook the speedometer cable (1) to the heater case.
7. Install the instrument cluster assembly. Refer to Instrument Cluster Replacement .