Lighting Systems Components. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Audio Alarm Module | Behind the RH instrument panel near the RH front speaker | -- | --
Backup Lamp Switch (Manual Transmission) | Mounted on the top of the transmission | -- | --
Cigar Lighter | Center of the instrument panel below the radio | -- | --
Combination Switch | On the steering column | Power and Grounding Component Views in Wiring Systems | --
Cruise Control ON/OFF Switch | LH instrument panel to the right of the steering column | Cruise Control Component Views in Cruise Control | --
Daytime Running Lamps (DRL) Control Module | Behind the instrument panel to the left of the steering column on the powertrain module mounting bracket | -- | --
Daytime Running Lamps (DRL) Diode | RH instrument panel taped to the main harness above the blower | -- | --
Dome Lamp Diode (2-door) | Taped to the floor harness near C407 | Lighting Systems Component Views | --
Dome Lamp Diode (4-door) | Taped to the floor harness near C407 | Lighting Systems Component Views | --
Fuse Block 1 | RH engine compartment in front of the battery | Power and Grounding Component Views in Wiring Systems | --
C1 (3 Cavities) | Main harness to fuse block 1 below fuse block 1 | Power and Grounding Component Views in Wiring Systems | --
Fuse Block 2 | Under the LH instrument panel | Power and Grounding Component Views in Wiring Systems | --
Generator | RH lower front of the engine | -- | --
Headlamp/ Dimmer Switch | LH steering column in the combination switch | -- | --
Headlamp Relay 1 | RH instrument panel behind the instrument panel compartment in front of the blower motor | Lighting Systems Component Views | --
Headlamp Relay 2 | RH instrument panel behind the instrument panel compartment in front of the blower motor | Lighting Systems Component Views | --
Illumination Controller | LH instrument panel to the left of the steering column | -- | --
Instrument Panel Cluster Assembly | LH instrument panel | -- | --
C1 (16 Terminals) | Instrument panel harness to the instrument panel cluster assembly behind the instrument panel cluster assembly | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges, and Console | --
C2 (10 Terminals) | Instrument panel harness to the instrument panel cluster assembly behind the instrument panel cluster assembly | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges, and Console | --
C3 (13 Terminals) | Instrument panel harness to the instrument panel cluster assembly behind the instrument panel cluster assembly | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges, and Console | --
LH Door Jamb Switch (2-Door) | Lower the LH B-Pillar | Lighting Systems Component Views | --
LH Front Door Jamb Switch (4-Door) | Lower LH B-Pillar | Lighting Systems Component Views | --
LH Rear Door Jamb Switch (4-Door) | LH C-Pillar above the wheelhousing | Lighting Systems Component Views | --
Parking Brake Switch | In the center console to the left of the parking brake | -- | --
Park/ Neutral Position (PNP) Switch (3-Speed Automatic Transmission) | RH side of the transmission | -- | --
C2 (4 Cavities) | Engine harness to PNP switch on the RH side of the transmission | -- | --
Powertrain Control Module (PCM) | Under the LH instrument panel to the left of the steering column | Engine Controls Component Views in Engine Controls - 1.6L | Powertrain Control Module Connector End Views in Engine Controls - 1.6L
Power/ Normal Switch (4-Speed Automatic Transmission) | In the center console to the right of the manual selector lever | -- | --
Radio | Center of the instrument panel | Entertainment Component Views in Entertainment | --
Rear Defogger Switch (4-Door) | LH instrument panel to the left of the steering column | -- | --
Rear Door Jamb Switch | LH bottom of the rear door jamb | Power Door Systems Component Views in Doors | --
Rear Wiper/ Washer Switch (4-Door) | LH instrument panel to the right of the steering column | Power and Grounding Component Views in Wiring Systems | --
RH Door Jamb Switch (2-Door) | Lower RH B-pillar | Power Door Systems Component Views in Doors | --
RH Front Door Jamb Switch (4-Door) | Lower RH B-pillar | -- | --
RH Rear Door Jamb (4-Door) | RH C-pillar above the wheelhousing | -- | --
Stoplamp Switch | Under the LH instrument panel above the brake pedal | Lighting Systems Component Views | --
Transmission Range Switch (4-Speed Automatic Transmission) | RH side of the transmission | -- | --
Turn/ Hazard Relay | Center instrument panel behind the blower speed selector | Lighting Systems Component Views | --
C100 (16 Cavities) | Main harness to the engine harness mounted to the bracket on the bulkhead to the left of the front wiper motor | Harness Routing Views in Wiring Systems | --
C101 (16 Cavities) | Main harness to the engine harness mounted to the bracket on the bulkhead to the left of the front wiper motor | Harness Routing Views in Wiring Systems | --
C104 (6 Cavities) (Manual and 3-Speed Automatic Transmission) | Engine harness to the transmission harness, RH rear of the engine under the intake manifold | Harness Routing Views in Wiring Systems | --
C104 (9 Cavities) (4-Speed Automatic Transmission) | Engine harness to the transmission harness, RH rear of the engine under the intake manifold | Harness Routing Views in Wiring Systems | --
C106 (10 Cavities) (4-Speed Automatic Transmission) | Engine harness to the transmission harness, RH rear of the engine under the intake manifold | Harness Routing Views in Wiring Systems | --
C200 (22 Cavities) | Main harness to the instrument panel harness, LH instrument panel near fuse block 2 | Harness Routing Views in Wiring Systems | --
C201 (16 Cavities) | Main harness to the instrument panel harness, LH instrument panel near fuse block 2 | Harness Routing Views in Wiring Systems | --
C211 (16 Cavities) | Instrument panel harness to the floor harness, RH instrument panel near the A-pillar | Harness Routing Views in Wiring Systems | --
C213 (6 Cavities) | Instrument panel harness to the shift illumination | Harness Routing Views in Wiring Systems | --
C215 (2 Cavities) (4-Door) | Main harness to the dome lamp harness, RH instrument panel near the A-pillar | Harness Routing Views in Wiring Systems | --
C300 (2 Cavities) (2-Door) | Floor harness to the dome lamp harness behind the LH rear passenger compartment trim panel | Harness Routing Views in Wiring Systems | --
C301 (6 Cavities) (2-Door) | Floor harness to the sub-floor harness behind the LH rear passenger compartment trim panel | Harness Routing Views in Wiring Systems | --
C400 (12 Cavities) | Floor harness to the rear lamp harness behind the LH rear wheelhousing | Harness Routing Views in Wiring Systems | --
C402 (6 Cavities) | Rear lamp harness to the RH rear combination lamp jumper harness behind the RH rear wheelhousing | Harness Routing Views in Wiring Systems | --
C403 (2 Cavities) (2-Door) | Rear lamp harness to the rear door harness behind the RH rear wheelhousing | Harness Routing Views in Wiring Systems | --
C404 (1 Cavity) | Rear lamp harness to the rear door harness behind the RH rear wheelhousing | Harness Routing Views in Wiring Systems | --
C405 (2 Cavities) (4-Door) | Rear door harness to the center high mount stoplamp jumper harness inside the rear door to the left of the license plate lamp connector breakout | Harness Routing Views in Wiring Systems | --
C405 (2 Cavities) (2-Door) | Rear door harness to the center high mount stoplamp jumper harness inside the center rear door | Harness Routing Views in Wiring Systems | --
C406 (6 Cavities) | Floor harness to the LH rear combination lamp jumper harness behind the LH rear wheelhousing | Harness Routing Views in Wiring Systems | --
C407 (6 Cavities) | Floor harness to the trailer option harness behind the LH rear wheelhousing | Harness Routing Views in Wiring Systems | --
G100 | LH front inner fender | Power and Grounding Component Views in Wiring Systems | --
G104 | RH front inner fender near the washer fluid reservoir | Power and Grounding Component Views in Wiring Systems | --
G200 | Behind the LH instrument panel above fuse block 2 | Power and Grounding Component Views in Wiring Systems | --
G201 | Behind the RH instrument panel near the blower assembly | Power and Grounding Component Views in Wiring Systems | --
G202 | Behind the center instrument panel on the bulkhead | Power and Grounding Component Views in Wiring Systems | --
G300 (4-Door) | LH rear passenger compartment behind the trim panel | Power and Grounding Component Views in Wiring Systems | --
G300 (2-Door) | LH rear passenger compartment behind the trim plate | Power and Grounding Component Views in Wiring Systems | --
G400 (4-Door) | Inside the rear door near the license plate lamps | Power and Grounding Component Views in Wiring Systems | --
G400 (2-Door) | Inside the rear door near the license plate lamps | Power and Grounding Component Views in Wiring Systems | --
G402 (2-Door) | Rear lamp harness behind the LH rear wheelhousing | Power and Grounding Component Views in Wiring Systems | --
P200 | LH rear engine compartment on the bulkhead near the brake master cylinder | Power and Grounding Component Views in Wiring Systems | --
P201 | RH rear engine compartment on the bulkhead near the battery | Power and Grounding Component Views in Wiring Systems | --
P300 (2-Door) | LH A-pillar under the instrument panel behind the LH kick panel | Power and Grounding Component Views in Wiring Systems | --
P400 (2-Door) | Rear door | Power and Grounding Component Views in Wiring Systems | --
P400 (4-Door) | Rear door | Power and Grounding Component Views in Wiring Systems | --
P401 | Rear of the vehicle to the right of the LH frame rail | Power and Grounding Component Views in Wiring Systems | --
P402 | Rear of the vehicle to the left of the RH frame rail | Power and Grounding Component Views in Wiring Systems | --
S103 | Main harness approximately 8 cm (3.14 in) from the right horn connectors breakout | Harness Routing Views in Wiring Systems | --
S115 | Main harness approximately 10 cm (3.93 in) from the evaporative canister vent control valve | Harness Routing Views in Wiring Systems | --
S116 | Main harness approximately 14 cm (5.51 in) from the LH bulkhead branch breakout | Harness Routing Views in Wiring Systems | --
S120 | Main harness approximately 15 cm (5.90 in) from the G100 breakout | Harness Routing Views in Wiring Systems | --
S140 | Main harness approximately 6 cm (2.36 in) from the noise suppressor filter connector breakout | Harness Routing Views in Wiring Systems | --
S204 | Instrument panel harness approximately 8 cm (3.14 in) from the C211 breakout | Harness Routing Views in Wiring Systems | --
S205 | Instrument panel harness approximately 12 cm (4.72 in) from the cigar lighter breakout | Harness Routing Views in Wiring Systems | --
S208 | Main harness approximately 18 cm (7.08 in) from the ignition switch connector breakout | Harness Routing Views in Wiring Systems | --
S210 | Main harness approximately 12 cm (4.72 in) from the stoplamp switch connector breakout | Harness Routing Views in Wiring Systems | --
S212 | Main harness approximately 6 cm (2.36 in) from the blower speed selector switch connector breakout | Harness Routing Views in Wiring Systems | --
S214 | Main harness approximately 10 cm (3.93 in) from the C216 connector | Harness Routing Views in Wiring Systems | --
S216 | Main harness approximately 2 cm (0.78 in) from the stoplamp switch connector breakout | Harness Routing Views in Wiring Systems | --
S220 | Main harness approximately 1 cm (0.39 in) from the blower speed selector switch connector breakout | Harness Routing Views in Wiring Systems | --
S221 | Instrument panel harness approximately 12 cm (4.72 in) from the cigar lighter breakout | Harness Routing Views in Wiring Systems | --
S222 | Main harness approximately 10 cm (3.93 in) from the blower speed selector switch connector breakout | Harness Routing Views in Wiring Systems | --
S225 | Instrument panel harness approximately 12 cm (4.72 in) from the cigar lighter | Harness Routing Views in Wiring Systems | --
S226 | Instrument panel harness near the radio breakout | Harness Routing Views in Wiring Systems | --
S227 | Main harness approximately 8 cm (3.14 in) from the stoplamp switch connector breakout | Harness Routing Views in Wiring Systems | --
S229 | Main harness approximately 7 cm (2.75 in) from the ignition switch connector breakout | Harness Routing Views in Wiring Systems | --
S230 | Main harness approximately 5 cm (1.96 in) from the G300 breakout | Harness Routing Views in Wiring Systems | --
S231 | Main harness approximately 1 cm (0.39 in) from the blower speed selector switch connector breakout | Harness Routing Views in Wiring Systems | --
S232 | Main harness approximately 1 cm (0.39 in) from the G200 breakout | Harness Routing Views in Wiring Systems | --
S241 | Main harness approximately 8 cm (3.14 in) from the powertrain control module (PCM) connectors breakout | Harness Routing Views in Wiring Systems | --
S243 | Main harness approximately 17 cm (6.69 in) from the G216 breakout | Harness Routing Views in Wiring Systems | --
S244 | Main harness approximately 25 cm (9.84 in) from the ignition switch connector breakout | Harness Routing Views in Wiring Systems | --
S246 | Main harness approximately 14 cm (5.51 in) from the ignition switch connector breakout | Harness Routing Views in Wiring Systems | --
S247 | Main harness approximately 2 cm (0.78 in) from the C212 breakout | Harness Routing Views in Wiring Systems | --
S250 | Main harness approximately 5 cm (1.96 in) from the blower motor resistor connector breakout | Harness Routing Views in Wiring Systems | --
S251 | Main harness approximately 5 cm (1.96 in) from the stoplamp switch connector breakout | Harness Routing Views in Wiring Systems | --
S254 | Main harness approximately 10 cm (3.93 in) from the G200 breakout | Harness Routing Views in Wiring Systems | --
S255 | Main harness approximately 16 cm (6.29 in) from the ignition switch connector breakout | Harness Routing Views in Wiring Systems | --
S256 | Instrument panel harness approximately 3 cm (1.18 in) from the power mirror switch connector breakout | Harness Routing Views in Wiring Systems | --
S257 | Main harness approximately 1 cm (0.39 in) from the stoplamp switch connector breakout | Harness Routing Views in Wiring Systems | --
S258 | Instrument panel harness approximately 2 cm (0.78 in) from the power mirror switch connector breakout | Harness Routing Views in Wiring Systems | --
S260 | Main harness approximately 4 cm (1.57 in) from the stoplamp switch connector breakout | Harness Routing Views in Wiring Systems | --
S262 | Main harness approximately 8 cm (3.14 in) from the stoplamp switch connector breakout | Harness Routing Views in Wiring Systems | --
S263 (4-Speed Automatic Transmission) | In the manual selector lever harness | Harness Routing Views in Wiring Systems | --
S265 (4-Speed Automatic Transmission) | In the manual selector lever harness | Harness Routing Views in Wiring Systems | --
S272 | Main harness approximately 11 cm (4.33 in) from the G200 breakout | Harness Routing Views in Wiring Systems | --
S275 | Main harness approximately 11 cm (4.33 in) from the ignition switch connector breakout | Harness Routing Views in Wiring Systems | --
S276 | Main harness approximately 1 cm (0.39 in) from the G200 breakout | Harness Routing Views in Wiring Systems | --
S282 | Main harness near G200 breakout | Harness Routing Views in Wiring Systems | --
S283 | Main harness approximately 8 cm (3.14 in) from the daytime running lamps (DRL) control module connector breakout | Harness Routing Views in Wiring Systems | --
S296 | Main harness approximately 6 cm (2.36 in) from the stoplamp switch connector breakout | Harness Routing Views in Wiring Systems | --
S297 | Main harness approximately 5 cm (1.96 in) from the daytime running lamps (DRL) diode connector breakout | Harness Routing Views in Wiring Systems | --
S300 (2-Door) | Floor harness approximately 10 cm (3.93 in) from the LH rear speaker connector breakout | Harness Routing Views in Wiring Systems | --
S301 (2-Door) | Sub-floor harness near the seat belt switch connector breakout | Harness Routing Views in Wiring Systems | --
S304 (2-Door) | Floor harness approximately 5 cm (1.96 in) from the LH rear speaker connector breakout | Harness Routing Views in Wiring Systems | --
S306 (2-Door) | Floor harness approximately 20 cm (7.87 in) from the LH rear speaker connector breakout | Harness Routing Views in Wiring Systems | --
S400 | Rear door harness near G400 breakout | Harness Routing Views in Wiring Systems | --
S401 | Rear lamp harness, near LH rear combination lamp | Harness Routing Views in Wiring Systems | --
S402 | Rear lamp harness, near RH rear combination lamp | Harness Routing Views in Wiring Systems | --
S403 | Rear lamp harness near the RH rear combination lamp | Harness Routing Views in Wiring Systems | --
S404 (2-Door) | Floor harness approximately 4 cm (1.57 in) from the C406 breakout | Harness Routing Views in Wiring Systems | --
S404 (4-Door) | Floor harness approximately 4 cm (1.57 in) from the LH rear speaker connector breakout | Harness Routing Views in Wiring Systems | --
S405 | Floor harness approximately 4 cm (1.57 in) from the G300 breakout | Harness Routing Views in Wiring Systems | --
S406 (4-Door) | Floor harness approximately 4 cm (1.57 in) from the G300 breakout | Harness Routing Views in Wiring Systems | --
S407 | Rear door harness near the license plate lamps | Harness Routing Views in Wiring Systems | --
S408 | Rear lamp harness near the LH rear combination lamp | Harness Routing Views in Wiring Systems | --
S409 (2-Door) | Floor harness approximately 5 cm (1.96 in) from the C406 breakout | Harness Routing Views in Wiring Systems | --
S409 (4-Door) | Floor harness approximately 30 cm (11.81 in) from the G300 breakout | Harness Routing Views in Wiring Systems | --
S410 | Rear door harness near the license plate lamps | Harness Routing Views in Wiring Systems | --
S411 (2-Door) | Floor harness approximately 2 cm (0.78 in) from the C406 breakout | Harness Routing Views in Wiring Systems | --
S411 (4-Door) | Floor harness approximately 2 cm (0.78 in) from the G300 breakout | Harness Routing Views in Wiring Systems | --
S412 (4-Door) | Floor harness approximately 42 cm (16.53 in) from the G300 breakout | Harness Routing Views in Wiring Systems | --
S413 (2-Door) | Floor harness approximately 10 cm (3.93 in) from the C406 breakout | Harness Routing Views in Wiring Systems | --
S413 (4-Door) | Floor harness approximately 30 cm (11.81 in) from the G300 breakout | Harness Routing Views in Wiring Systems | --
S414 | LH rear combination lamp jumper near the LH rear combination lamp | Harness Routing Views in Wiring Systems | --
S415 | RH rear combination lamp jumper near the RH rear combination lamp | Harness Routing Views in Wiring Systems | --
S416 | Rear lamp harness near the RH rear combination lamp connector breakout | Harness Routing Views in Wiring Systems | --
S417 | Floor harness 1 near the LH rear wheel housing | Harness Routing Views in Wiring Systems | --
S418 (2-Door) | Floor harness approximately 3 cm (1.18 in) from the C406 breakout | Harness Routing Views in Wiring Systems | --
S418 (4-Door) | Floor harness approximately 25 cm (9.84 in) from the G300 breakout | Harness Routing Views in Wiring Systems | --
S422 (4-Door) | Floor harness approximately 7 cm (2.75 in) from the G300 breakout | Harness Routing Views in Wiring Systems | --
S423 (4-Door) | Floor harness approximately 8 cm (3.14 in) from the G300 breakout | Harness Routing Views in Wiring Systems | --
S424 (4-Door) | Floor harness approximately 10 cm (3.93 in) from the C406 breakout | Harness Routing Views in Wiring Systems | --
S426 (4-Door) | Floor harness approximately 20 cm (7.87 in) from the G300 breakout | Harness Routing Views in Wiring Systems | --