Instrument Cluster Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the hazard lamps switch by gently pulling the knob straight up.
3. Remove the instrument cluster bezel from the instrument panel. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement .
4. Remove the 4 screws and pull the instrument cluster assembly forward from the instrument panel.
5. Disconnect the 3 electrical connectors.
6. Remove the speedometer cable at the speedometer head.
7. Remove the instrument cluster assembly from the vehicle.

### Installation Procedure

1. Connect the 3 electrical connectors and install the speedometer cable to the instrument cluster assembly.
2. Install the instrument cluster assembly to the instrument panel. Secure the cluster assembly with the 4 screws.
3. Install the instrument cluster bezel to the instrument panel. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement .
4. Push into place the hazard lamps switch knob.
5. Connect the negative battery cable.