Front Side Door Lock Striker Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Mark the position of the front side door lock striker (4) on the door jamb for ease of installation.
2. Remove 2 screws and the front side door lock striker (4) from the door jamb.

### Installation Procedure

1. Install the front side door lock striker (4) to the door jamb. Secure the striker with 2 screws.
2. Adjust the striker vertical measurement so that the striker (1) shaft aligns with the center of the door lock (2).
3. Adjust the lock striker (1)-to-door distance to 13-15 mm (0.51-0.59 in) by installing or removing shims (2) as necessary.
4. Keeping the lock striker (1) level, move the striker sideways in order to adjust door flushness with the quarter panel (3) on 2 door models or the door jamb (3) on 4 door models. Refer to Door Adjustment Specifications .