Wheel Alignment - Steering Wheel Angle and/or Front Toe Adjustment. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Use the following steps in order to adjust the toe:

1. Loosen the locknuts.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Rotate the left and the right tie rods by the same amount.

Rotate the left and the right tie rods until the toe-in measures 0.16-0.48 degrees.

Ensure that the right and the left tie rods become equal in length.

Tighten
Tighten tie rod locknuts to 65 N·m (48 lb ft).