Door Lock Cylinder Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the front side door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the screws and the door trim support bracket from the door.
3. Peel the water deflector (1) from the door.
4. Remove the front side door lock cylinder lock rod (6) from the lock cylinder (11).
5. Remove the front side door lock cylinder retaining clip.
6. Remove the front side door lock cylinder (11) from the door.

### Installation Procedure

1. Install the front side door lock cylinder (11) to the door. Secure the front side door lock cylinder (11) with the retaining clip.
2. Install the front side door lock cylinder lock rod (6) to the lock cylinder (11).
3. Inspect the water deflector (1) for tears and holes.
4. In order to repair the tears or holes, use waterproof tape on both sides of the water deflector (1), as needed.
5. Apply adhesive (2) to the back of the water deflector (1).
6. Install the water deflector (1) to the door.
7. Install the door trim support bracket to the door. Secure the bracket with the screws.
8. Install the front side door trim panel. Refer to Front Side Door Trim Panel Replacement .