Hazard and Turn Signal Flasher Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Pull out the instrument panel compartment while pushing the stopper from both the left and right sides.
3. Remove the 2 screws wich secure the relay mounting bracket.

Important: Refer to Headlights/Daytime Running Lights (DRL) Schematics for proper identification of the turn/hazard relay.

4. Remove the relay mounting bracket from the heater case.
5. Remove the turn/hazard relay from the mounting bracket by releasing the locking tab.
6. Disconnect the turn/hazard relay electrical connector.
7. Remove the turn/hazard relay from the vehicle.

### Installation Procedure

1. Connect the turn/hazard relay electrical connector.
2. Install the turn/hazard relay to the mounting bracket.
3. Install the relay mounting bracket to the heater case. Secure the relay mounting bracket with the 2 screws.
4. Close the instrument panel compartment.
5. Connect the negative battery cable.