Detent Valve Assembly Removal. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

1. Remove the detent valve retaining pin (112) using diagonal pliers. Insert a wire into the center of the spring pin to prevent collapsing.
2. Remove the detent valve sleeve (111) and seal (113).
3. Remove the detent valve (110).
4. Remove the detent valve spring (108).
5. Inspect the detent valve sleeve for:

• | nicks

• | scratches

• | scoring

6. Inspect the detent valve and the valve spring for:

• | nicks

• | scratches

• | scoring