Front Lower Control Arm Bushing Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

#### Tools Required

• | J 35561 Front Control Arm Bushing Service Set

• | J 29792 Front Control Arm Bushing Service Set

• | J 9519-7 Bearing Remover

• | J 9519-17 Bearing Remover

1. Remove the control arm from the vehicle. Refer to Lower Control Arm Replacement in this section.
2. Use the J 35561 installer, the J 29792 receiver and a press (1) in order to remove the bushing (2) from the short branch (3) of the control arm.
3. Use the J 29792 installer, the J 9519-7 , the J 9519-17 and a press (1) in order to remove the bushing from the long branch (2) of the control arm.

### Installation Procedure

#### Tools Required

• | J 35561 Front Control Arm Bushing Service Set

• | J 29792 Front Control Arm Bushing Service Set

• | J 9519-16 Bearing Installer

• | J 9519-9 Bearing Installer

1. Use the J 35561 installer, the J 29792 receiver and a press (1) in order to install a new bushing (2) into the short branch (3) of the control arm.
2. Use the J 29792 installer, the J 9519-9 , the J 9519-16 and a press (1) in order to install a new bushing (3) into the long branch (2) of the control arm.
3. Install the control arm to the vehicle. Refer to Lower Control Arm Replacement in this section.