Wipers Delay Mode Inoperative. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Wiper/Washer System Check? | -- | Go to Step 2 | Go to Wiper/Washer System Check

2

1. Turn the ignition switch to the LOCK position.
2. Disconnect the combination switch.
3. Connect a J 39200 digital multimeter (DMM) from combination switch connector cavity 7 to ground.
4. Measure the resistance.

Is the measured resistance more than the specified value?

1.0 ohms

Go to Step 3

Go to Step 4

3 | Repair the open in the BLK wire between the combination switch and G202. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Wiper/Washer System Check | --
4 | Replace the combination switch. Refer to Windshield Wiper and Washer Switch Replacement . Is the repair complete? | -- | Go to Wiper/Washer System Check | --