Front Side Marker Lamp Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Gently pry the front end of the front side marker lamp (2) from the body in order to disengage the retaining clip.
2. Remove the front side marker lamp bulb socket (1) from the front side marker lamp (2).
3. Remove the bulb from the socket, as needed.

### Installation Procedure

1. Install the bulb to the socket, if removed.
2. Install the front side marker lamp bulb socket (1) to the front side marker lamp (2).
3. Install the front side marker lamp to the vehicle.
4. Gently push the front side marker lamp securely against the body in order to engage the retaining clip.