Dome Lamp Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Gently pry the dome lamp lens (2) from the dome lamp assembly (1) with a flat-bladed screwdriver.
2. Remove the dome lamp bulb from the dome lamp assembly, if necessary.
3. Remove the 2 screws which secure the dome lamp assembly.
4. Lower the dome lamp assembly (1) from the headlining.
5. Disconnect the dome lamp electrical connector.
6. Remove the dome lamp assembly (1) from the vehicle.

### Installation Procedure

1. Connect the dome lamp electrical connector.
2. Install the dome lamp assembly (1) to the headlining. Secure the dome lamp with the 2 screws.
3. Install the dome lamp bulb to the dome lamp assembly (1), if removed.
4. Install the dome lamp lens (2) to the dome lamp assembly (1).

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

5. Connect the negative battery cable.