Wipers Always On. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Wiper Washer System Check? | -- | Go to Step 2 | Go to Wiper/Washer System Check

2

1. Turn the ignition switch ON.
2. Pull the front wiper/washer switch toward the driver's seat and release.
3. Disconnect the combination switch connector.

Do the wipers stop operating?

--

Go to Step 3

Go to Step 4

3 | Replace the combination switch. Refer to Windshield Wiper and Washer Switch Replacement . Is the repair complete? | -- | Go to Wiper/Washer System Check | --

4

1. Disconnect the front wiper motor connector.
2. Connect a J 35616-200 unpowered test lamp from the front wiper motor connector cavity 2 to ground.

Did the test lamp light?

--

Go to Step 5

Go to Step 6

5 | Repair the short to voltage in the BLU wire between the combination switch and the front wiper motor. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Wiper/Washer System Check | --
6 | Test for a short to voltage in the BLU/RED wire between the combination switch and the front wiper motor. Is there a short to voltage? | -- | Go to Step 7 | Go to Step 8
7 | Repair the short to voltage between the BLU/RED wire between the combination switch and the front wiper motor. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Wiper/Washer System Check | --
8 | Test for a short to voltage in the BLU/WHT wire between the combination switch and the front wiper motor. Is there a short to voltage? | -- | Go to Step 9 | Go to Windshield Wiper Motor Replacement
9 | Repair the short to voltage between the BLU/WHT wire between the combination switch and the front wiper motor. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Wiper/Washer System Check | --