Rear Window Reveal Molding Replacement - Right Side. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Unsnap the rear garnish (3) from the lower right side of the rear door.
2. Pull the upper right-side reveal molding joint (1) from the rear door.
3. Pull the right-side reveal molding (2) from the rear door.

### Installation Procedure

Important: Trim the new right-side reveal molding (2), as needed, in order to fit the right-side reveal molding (2) in the cavity between the rear door and window.

1. Apply a bead of urethane adhesive from the kit GM P/N 12346284 into the cavity between the body and the window.
2. Install the right-side reveal molding (2) to the rear door.
3. Start at the center of the right-side reveal molding (2) in order to press the right-side reveal molding (2) in place.
4. Press the upper right-side upper reveal molding joint (1) to the rear door.
5. Use tape, as needed, in order to retain the right-side reveal molding (2) until the urethane cures.
6. Allow the adhesive to cure according to the manufacturer's instructions.
7. Install the rear garnish (3) to the lower right side of the rear door.