Lamp Driver Relay Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

The lamp driver relay is located on the left hand side of the engine compartment, on the inner fender next to the hydraulic modulator.

1. Pull the lamp driver relay (1) from the mounting bracket.
2. Disconnect the lamp driver relay electrical connector.

### Installation Procedure

1. Connect the lamp driver relay electrical connector.
2. Install the lamp driver relay (1) to the mounting bracket.
3. Perform the Diagnostic System Check .