Poor Return of Steering Wheel. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Inspect the following components and the following conditions:

• | The wheel alignment

• | The wheel bearings for wear or damage

• | The joints from the column to the steering gear for free movement

• | The joints from the column to the steering gear for proper installation

• | The tie rod ends for free movement

• | The ball joints for free movement

• | The steering shaft bearings for free movement

• | The steering gear adjustment

• | The steering gear valve for the proper operation

• | The ball studs for lack of lubrication

• | The tie rod ends for lack of lubrication

• | The ball studs for binding

• | The steering column for binding

• | The steering gear valve for sticking and proper operation

• | The steering gear adjustment

• | The steering gear for binding on the lower coupling

• | The tires for adequate inflation