Electrical Center Identification Views. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

#### Fuse Block 2

Fuse/Circuit Breaker | Rating | Description
--- | --- | ---

Cigar Radio Fuse

20 A

• | Cigar Lighter

• | Power Mirror Switch

• | Radio

Door Lock Fuse | 20 A | Power Lock Control Module
Hazard Fuse | 15 A | Combination Switch

Heater Fuse

25 A

• | A/C Amplifier

• | Blower Speed Selector Switch

• | Dual Pressure Switch

IG-Coil Meter Fuse

15 A

• | Audio Alarm Mode

• | Cruise Control On/Off Switch

• | Daytime Running Lamps (DRL) Control Module

• | Distributor

• | Fuel Pump Relay

• | Generator

• | Heated Oxygen Sensor 1 (HO2S1)

• | Heated Oxygen Sensor 2 (HO2S1)

• | Instrument Cluster Assembly

• | Lamp Driver Relay

• | Main Relay

• | Noise Suppressor Filter

• | Torque Converter Clutch (TCC) Relay

Power Windows Circuit Breaker

50 A

• | LH Front Power Window/Door Lock Switch

• | LH Rear Power Window Switch

• | LH Rear Remote Power Window Switch

• | RH Front Power Window Switch

• | RH Rear Power Window Switch

• | RH Rear Remote Power Window Switch

Rear Defog Fuse

15 A

• | Electronic Brake Control Module (EBCM)

• | Electronic Brake Control Relay

• | Rear Defogger Switch

Tail Dome Fuse

15 A

• | Data Link Connector-On Board Diagnostics II (DLC-OBD II)

• | Dome Lamp

• | Electronic Brake Control Module (EBCM)

• | Headlamp Relay 2

• | Ignition Key Warning Switch

• | Powertrain Control Module (PCM)

• | Radio

• | Spot Lamp (Not Used)

Turn Back Fuse

15 A

• | Antilock Brake System (ABS) Resistor

• | Backup Lamp Switch

• | Combination Switch

• | Park/Neutral Position (PNP) Switch

• | Transmission Range Switch

Wiper/Washer Fuse

15 A

• | Combination Switch

• | Front Wiper Motor

• | Rear Wiper Motor (4-Door)

• | Rear Wiper/Washer Switch (4-Door)

• | Shift Lock Relay (Automatic Transmission)

#### Fuse Block 1

Fuse/Circuit Breaker | Rating | Description
--- | --- | ---

A/C Fuse

25 A

• | A/C Compressor Clutch Relay

• | A/C Compressor Fan Relay

ABS Fuse | 50 A | Electronic Brake Control Relay
BAT Fuse | 80 A | From Battery Positive (+) to Generator
FL Fuse | 15 A | Main Relay
IG | 60 A | Main Harness Connector C3
Lamp | 30 A | Main Harness Connector C4

Left Headlamp Fuse

15 A

• | Daytime Running Lamps (DRL) Diode

• | Instrument Panel Cluster Assembly

• | LH Headlamp

Right Headlamp Fuse

15 A

• | Daytime Running Lamps (DRL) Diode

• | RH Headlamp

#### Air Bag Fuse Box

Fuse/Circuit Breaker | Rating | Description
--- | --- | ---
SIR IG Fuse | 15 A | Inflatable Restraint Sensing and Diagnostic Module