Rear Wiper Inoperative. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Wiper/Washer Rear System Check? | -- | Go to Step 2 | Go to Wiper/Washer Rear System Check

2

1. Turn the ignition switch to ON.
2. Press the rear wiper switch to ON.
3. Backprobe the rear wiper/washer switch connector with a J 35616-200 unpowered test lamp from cavity 4 to ground.

Did the test lamp light?

--

Go to Step 3

Go to Step 4

3 | Backprobe the rear wiper/washer switch connector with a J 35616-200 unpowered test lamp from cavity 1 to ground. Did the test lamp light? | -- | Go to Step 6 | Go to Step 5
4 | Repair the open in the YEL/BLU wire between fuse block 2 and the rear wiper/washer switch. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Wiper/Washer Rear System Check | --
5 | Replace the rear wiper/washer switch. Refer to Windshield Wiper and Washer Switch Replacement . Is the repair complete? | -- | Go to Wiper/Washer Rear System Check | --
6 | Backprobe the rear wiper motor connector with a test lamp from cavity 4 to ground. Did the test lamp light? | -- | Go to Step 7 | Go to Step 8
7 | Replace the rear wiper motor. Refer to Rear Window Wiper Motor Replacement . Is the repair complete? | -- | Go to Wiper/Washer Rear System Check | --
8 | Repair the open in the ORN wire between the rear wiper/washer switch and the rear wiper motor. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Wiper/Washer Rear System Check | --