Front Seat Cushion Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the front seat from the vehicle. Front Seat Replacement - Bucket .
2. Remove the front seatback (9) from the seat cushion (6). Refer to Front Seat Back Replacement .
3. Remove the 2 bolts which secure each front seat adjuster (5).
4. Remove the adjusters (5) from the front seat cushion (6).

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the seat adjusters (5) to the front seat cushion (6). Secure each seat adjuster (1) with 2 bolts.

Tighten
Tighten the front seat adjuster-to-front seat cushion bolts to 25 N·m (19 lb ft).

2. Install the front seatback (9) to the seat cushion (6). Refer to Front Seat Back Replacement .
3. Install the front seat to the vehicle. Refer to Front Seat Replacement - Bucket .