Reveal Molding Replacement - Rear Window Upper. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Pull the upper reveal molding joints (2, 6) from the left and right sides of the rear door.
2. Pull the upper reveal molding (8) from the rear door.

### Installation Procedure

Important: Trim the upper reveal molding (8), as needed, in order to fit in the cavity between the body and the window (7).

1. Apply a bead of urethane adhesive from the kit GM P/N 12346284 into the cavity between the body and the window.
2. Install the upper reveal molding (8) to the rear door.
3. Start at the center of the upper reveal molding (8) in order to press the upper reveal molding (8) into place.
4. Press the upper reveal molding left and right joints (2, 6) into place.
5. Use tape, as needed, in order to retain the reveal molding until the urethane cures.
6. Allow the adhesive to cure according to the manufacturer's instructions.