Transmission Fluid Pump Assemble. Pontiac Sun Runner - 2WD (Canada) 1997

For 1990-2009 cars

#### Tools Required

J 36850 Transjel®

1. Lubricate the valve with DEXRON®III automatic transmission fluid.
2. Install the pressure regulator valve (216).
3. Install the pressure regulator valve spring (215) and spring seats (214).
4. Install the oil pump boost valve (213) into the boost valve sleeve.
5. Install the oil pump boost valve sleeve (212).
6. Install the oil pump boost valve sleeve retainer pin (211).
7. Lubricate the valves with DEXRON®III automatic transmission fluid.
8. Install the clutch control valve (217).
9. Install the clutch control valve spring (218).
10. Install the control valve bore plug (219).
11. Install the converter clutch control valve bore plug retainer pin (220).
12. Install the second clutch oil seal rings (225).
13. Install the oil pump outer seal (223).
14. Install the oil pump to case gasket (207). Retain with J 36850 Transjel® or equivalent.