Backup Lamp Inoperative - One Lamp. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Backup Lights System Check? | -- | Go to Step 2 | Go to Backup Lamp System Check
2 | Is the left backup lamp the only inoperative component? | -- | Go to Step 4 | Go to Step 3
3 | Is the right backup lamp the only inoperative component? | -- | Go to Step 5 | --
4 | Test for an open in the RED wire between S418 and the left rear combination lamp. Is there an open? | -- | Go to Step 6 | Go to Step 7
5 | Test for an open in the RED wire between S418 and the right rear combination lamp. Is there an open? | -- | Go to Step 6 | Go to Step 8
6 | Repair the open. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Backup Lamp System Check | --
7 | Repair the open in the BLK wire between the left rear combination lamp and G300. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Backup Lamp System Check | --
8 | Repair the open in the BLK wire between the right rear combination lamp and G300. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Backup Lamp System Check | --