Fastener Tightening Specifications. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Battery

- Battery Hold Down Bracket Nuts

8 N·m

71 in ft

- Body Ground Bolt

14 N·m

124 in ft

- Fuse Box Bolt

10 N·m

89 in ft

- Generator Retaining Nut

8 N·m

71 in ft

- Ground Bolt

23 N·m

17 lb ft

- Negative (-) Battery Cable-to-Battery Terminal

5.5 N·m

48.68 in ft

- Positive (+) Battery Cable-to-Battery Terminal

5.5 N·m

48.68 in ft

- Positive (+) Battery Cable-to-Starter Solenoid Retainer Nut

7 N·m

62 in ft

Charging System

- Battery Terminal Retaining Nut

10 N·m

89 in ft

- Drive Belt Adjusting Bolt

33 N·m

24 lb ft

- Drive Pulley Retaining Nut

65 N·m

48 lb ft

- Generator Housing Bolts

17 N·m

10 lb ft

- Generator Lower Pivot Mounting Bolts

33 N·m

24 lb ft

- Generator Rectifier Nut

33 N·m

24 lb ft

- Generator Upper Mounting Bracket Bolts

27 N·m

20 lb ft

- Negative (-) Battery Cable-to-Negative Battery Terminal Retainer

5.5 N·m

48.68 in ft

Cranking System

- Commutator End Housing Bolts

30 N·m

22 lb ft

- Field Coil lead Wire Nut

15 N·m

11 lb ft

- Negative (-) Battery Cable-to-Negative (-) Battery Terminal Retainer

5.5 N·m

48.68 in ft

- Starter Motor Assembly Lower Mounting Nut

30 N·m

22 lb ft

- Starter Motor Assembly Upper Mounting Bolt and Retaining Nut

30 N·m

22 lb ft

- Starter Solenoid Nut

15 N·m

11 lb ft

Ignition System

- Spark Plugs

28 N·m

21 lb ft

- Distributor Flange Bolt

20 N·m

15 lb ft

- Negative (-) Battery Cable-to-Negative (-) Battery Terminal Retainer

5.5 N·m

48.68 in ft