Quarter Upper Trim Panel Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat belt guide loop cover.
2. Remove the rear seat belt guide loop anchor bolt (14).
3. Loosen the rear door opening weatherstrip (1).
4. Loosen the rear side door opening weatherstrip (11).
5. Remove the seat belt retractor trim panel (7).
6. Remove the 2 screws and the rear side upper trim panel.
7. Remove the 2 screws (4) and the rear quarter window interior trim (13) from the vehicle.

### Installation Procedure

1. Install the rear quarter window interior trim (13) to the vehicle. Secure the trim with the 2 screws (4).
2. Install the rear side upper trim panel. Secure the panel with the 2 screws.
3. Install the seat belt retractor trim panel (7).
4. Press the rear side door opening weatherstrip (1) into place.
5. Press the rear door opening weatherstrip (11) into place.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

6. Install the rear seat belt guide loop anchor bolt (14).

Tighten
Tighten the rear seat belt guide loop anchor bolt to 45 N·m (33 lb ft).

7. Install the rear seat belt guide loop cover.